**QUESTION:** Should Camera Control take pictures whenever it can or should something order it to take pictures when it needs (HINT HINT GNC)

**ANSWER:** Camera Controller will decide when it can take pictures by receiving the angular velocity of the Spacecraft.

**QUESTION:** Camera Controller knows when it can take a picture but does it always need to take a picture when it can take a picture?

**ANSWER:** No, Request Response, only when GNC asks it to take a picture.

**QUESTION:** Potentially combined Image Processing and Camera Controller into 1 process to avoid sending 20 MB message (Assume 100 MB per second connection between processes)

**ANSWER:** TBD much later down the road

**QUESTION:** Do we want to have our own Matrix / Vector class with simple methods built in?

**ANSWER:** Yes!